Simple bootNotification example of OCPP using python:

[GitHub - mobilityhouse/ocpp: Python implementation of the Open Charge Point Protocol (OCPP).](https://github.com/mobilityhouse/ocpp)

OCPP and other standard protocols used in EV industry:

[The EV Charging Industry Protocols and Standards list (driivz.com)](https://driivz.com/blog/ev-charging-standards-and-protocols/)

EV charging station standards in India:

[A Guide to EV Charging and EV Standards in India • EVreporter](https://evreporter.com/guide-to-ev-charging-and-standards-in-india/)

OCPP benefits:

[OCPP: connecting EV charging stations to central systems. (codibly.com)](https://codibly.com/news-insights/ocpp-connecting-ev-charging-stations-to-central-systems/)

A closer look of OCPP protocol:

[OCPP: connecting EV charging stations to central systems. (codibly.com)](https://codibly.com/news-insights/ocpp-connecting-ev-charging-stations-to-central-systems/)

OCPP with MQTT:

[Implementing OCPP over MQTT (iwheels.co)](https://iwheels.co/blog/implementing-ocpp-over-mqtt/#:~:text=Protocol%20Buffer%20is%20used%20to,of%20networks%20communication%20to%20MQTT.&text=We%20can%20use%20MQTT%20for,is%20based%20on%20TCP%2FIP.)

OCPP implementation in Arduino:

[GitHub - matth-x/ArduinoOcpp: OCPP 1.6 client for ESP32 / ESP8266](https://github.com/matth-x/ArduinoOcpp)